Installation into C++ Builder.

This information is also available in the file BuilderInstall.txt in the
installation directory.

C++ Builder 6:
Select the menu Component->Install packages, click the Add button. Browse to
the installation directory. Select the Package\CPP6 sub directory. Select the file
XLSRWII5_CPP6.bpl

C++ Builder 5:
Select the menu Component->Install packages, click the Add button. Browse to
the installation directory. Select the Package\CPP5 sub directory. Select the file
XLSRWII5_CPP5.bpl

*******************************************************************************  
******************************* IMPORTANT! ************************************
*******************************************************************************  

If installing into an new, empty package in C++ Builder, do this:

1. In the Package Manager, select the Requires node, right-click and
   choose Add to add DesignIDE.bpi (CPP6) or DsnIDE50. (CPP5)
2. Edit the XML source of the package by choosing Project|Edit Option Source.
3. In the source displayed, change the PFLAGS setting by adding an -LU switch
   to make the PFLAGS line look something like the following:

   CPP6: <PFLAGS value="-$YD -$W -$O- -v -JPHNE -M -LUDesignIde"/>
   CPP5: <PFLAGS value="-$YD -$W -$O- -v -JPHNE -M -LUdsnide50"/>
